1)Once alarm occur infinite box will end command 88 to machine software via dual ftdi.
2)Machine software receive command 88 - capture sceen and save to infinite box database via dual ethernet USB.
3)Infinite box detected new record ceated - save image to RawAlarm folder
4)Alarm will be recognized and sent to PAC